# Advanced Lifting

This method is recommended.

Reason:

- Advanced Lifting permits a greater lifting height to be reached.
- It increases collision protection.
- Advanced Lifting has no negative impact on lifting height caused by changes in feed rate or path override.
- Conventional lifting may result in Z axis overload.

Exception: A Type 3 slope is used or less computing time is required for technical reasons.

## Additional information

- Advanced Lifting properties
- Parameterisation
- Special cases