# Inner rectangle

After positioning in the pocket, the tough probe measures in the position and negative X and Y directions and uses the measured values to calculate the centre point.

The touch probe must be positioned at measuring depth as centrally as possible in the pocket either manually or in automatic mode.

Inner rectangle

## Additional information

- Process (internal cycle)
- Parameters
- Syntax
- Programming example
- Output variables