# ID 310005

Activation of distance control not possible because axis is part of active measurement.
Description | With axis-specific distance control, the axis to be controlled is still actively involved in a measurement when distance control was activated. With 3D distance control, an axis to be controlled is still involved in the measurement.
Response | Class | 7 | Controlled halt of the axis, the control loop is closed.
Solution | Class | 6 | Check and modify the process. Only activate distance control after measurement.
Parameter | %1: | Logical axis number [-] or Logical channel number [-]
Logical axis number Axis parameters of the axis affected for axis-specific distance control, logical channel number Logical number of a NC channel (P-CHAN-00400) for 3D distance control.
%2: | Error value [-]
Distance control state
%3: | Block number [-]
Block number that activates distance control.
%4: | Current value [-]
Error type | -