# ID 60207

Measure not allowed when already enabled or abort enabled.
Description | A measuring process (PLC-block MC_TouchProbe) was commanded for this axis although a measuring process or the abort of a measuring process is already active.
Response | Class | 6 | PLC module reports an error.
Solution | Class | 6 | Restart measuring only if preceding command is finished respectively aborted.
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle.
%2: | Current value [-]
Commanded measuring channel.
Error type | -