# Measure angle between drilled hole and spigot (C axis)

The centre point of the drilled hole is calculated by 4 measured points (see SysMeasWcs8, SysMeasWcs10) and by the angle between the drilled holes in relation to the X axis.

The touch probe must be positioned as centrally as possible above the first drilled hole either manually or in automatic mode.

If no C axis is configured, call the cycle without transferring @P7. The twist in C can be manually transferred to the related zero offset by evaluating the output variables in the post-program.

Measure angle between drilled hole and spigot (C axis)

## Additional information

- Process (internal cycle)
- Parameters
- Syntax
- Programming example
- Output variables