# Resolution of spindles (P-CHAN-00083)

P-CHAN-00083 | Resolution of spindles
Description | This value represents the conversion factor between the positions programmed in the NC program and the internal representation of positional values for spindles (M19).
Parameter | spind_aufloes
Data type | REAL64
Data range | 0 < spind_aufloes < MAX(REAL64)
Dimension | ----
Default value | 10000
Remarks | This resolution is used for regulated and controlled spindles. It is used only for positional values (M19) and not for speeds. Not to be confused with the resolution of the drive encoder P-AXIS-00234/P-AXIS-00235. As of CNC Build V2.11.2026.09 P-CHAN-00315 replaces the parameters lin_aufloes, rund_aufloes and spind_aufloes (P-CHAN-00034, P-CHAN-00035 and P-CHAN-00036). It is recommended to use only P-CHAN-00315 as of this CNC Build.

Parameterisation example: All spindles are specified in the dimension 'degree' [°] in the NC program.

spind_aufloes 10000

Internal representation in [0.0001°] | Typical value for spindle resolution | Programmed value in the NC program in [°]
10 000 [0.0001 °] | 10 000 | 1 [°]