# Parameters

Cycle parameters | Description
@P5 | Measurement path in the Y axis (incremental) Positive value, the touch probe moves in positive Y direction Negative value, the touch probe moves in negative Y direction
@P7 (optional) | Zero offset to be described (TCS) G54 to G59 Input without address “G” If not specified, then measurement only but no write function
@P12 (optional) | Reference angle [degrees] Default value = 0
@P17 | Pre-position along the X axis before the 2nd measurement
@P18 (optional) | Pre-position along the Y axis before the 2nd measurement Default value = 0

@P17 may not be 0.