# List interpretation with active NC program (P-CHAN-00146)

P-CHAN-00146 | Adopt configuration lists when NC program is active
Description | Normally, configuration lists may not be adopted when an NC program is active. This parameter can cancel this blocking. The user must then make sure that channel buffering is cancelled at the time when a new list is adopted by suitable programmed (e.g. #FLUSH WAIT in connection with an M function).

This allows the adoption of zero offsets, position offsets, tool data, external variables and channel parameters when an NC program is active.

Parameter | parameter_change_during_execution
Data type | BOOLEAN
Data range | 0: List interpretation blocked when an NC program is active (default). 1: List interpretation allowed when an NC program is active.
Dimension | ----
Default value | 0
Remarks |