# Additional error information value 1 - 5

Additional error information
Description | Individual error information
ST path | gpCh[channel_idx]^.mc_error.satz_r.rumpf.wert_1 ... wert_5
Data type | HLI_WERT_B
Description | Data type
ST path | .typ
Data type | INT
Value range | See Value range of variable ‘Type’ of additional error information
Description | Dimension of datum
ST path | .dimension
Data type | INT
Value range | See Value range of ‘Dimension’ variable of the additional error information
Description | Significance of datum
ST path | .bedeutung
Data type | INT
Value range | See Value range of ‘Significance’ variable of additional error information.
Description | Datum itself
ST path | .inhalt.data
Data type | ARRAY [0..HLI_WERT_B_DATA_MAXIDX] OF BYTE (as union, must be output type-caste corresponding to data type)

## Additional information

- Value range of variable ‘Type’ of additional error information
- Value range of ‘Dimension’ variable of the additional error information
- Value range of ‘Significance’ variable of additional error information