# ID 310023

During deselection of distance control, it was activated again.
Description | Distance control was deactivated and then re-activated immediately afterwards. After deactivation, wait until the existing compensation offset has finished before re-activating distance control. Alternatively, distance control can be disabled with the addition NO_MOVE without clearing the existing compensation offset.

See:

- Programming axis-specific distance control
- Programming 3D distance control

Response | Class | 7 | Controlled halt of the axis, the control loop is closed.
Solution | Class | 6 | Check and modify the process. Possibly disable distance control using OFF NO_MOVE to avoid clearing the existing compensation offset.
Parameter | %1: | Logical axis number [-] or Logical channel number [-]
Logical axis number Axis parameters of the axis affected for axis-specific distance control, logical channel number Logical number of a NC channel (P-CHAN-00400) for 3D distance control.
%2: | Block number [-]
Block number in the NC program
Error type | -