# Process (internal cycle)

1. Measurements in Z direction
2. After the start of the cycle, position the touch probe manually above the 1st measuring point.
3. Press Start again to start the measurement run.
4. Repeat this process with point 2 and point 3.
5. Then lift to the security distance @P13.
6. The orientation of the top surface is calculated and axes A, B and C are swivelled in.
7. Measurements in X direction
8. Then approach starting point 4 and press Start again.
9. Afterwards, approach starting point 5 and press Start again.
10. The measurement direction is determined from these points and positions 4 and 5 are measured automatically.
11. Measurements in Y direction
12. Approach point 6 manually and press Start.
13. Finally, approach point 7 manually and press Start.
14. The measurement direction is determined from these points and positions 6 and 7 are measured automatically.
15. A new file is written CS_BASE_[CS ID @P39].bcs

## Attention

If the file already exists, it is deleted and a new file is written. No back-up is made!