# ID 50119

Warning level of axis velocity exceeded.
Description | The maximum axis velocity set in the axis parameter list (P-AXIS-00212) was exceeded. Dynamic look-ahead also considers the warning threshold defined by the parameter P-AXIS-00439.
Response | Class | 1 | None
Solution | Class | 1 |
Parameter | %1: | Logical axis number [-]
Logical axis number (P-AXIS-00016) of axis affected.
%2: | Current value [1µm/s or 0.001°/s]
Current nominal velocity of the axis.
%3: | Upper limit value [1µm/s or 0.001°/s]
Maximum permissible velocity of the axis (P-AXIS-00212).
%4: | Current value [-]
Ratio of current velocity to maximum permissible axis velocity (absolute value).
%5: | Upper limit value [-]
Factor for permissible excess of velocity (P-AXIS-00439).
Error type | 1, Error message from NC program.