# ID 70207

Error reaction (CNC_controlled_stop_after_error) of master-/slave axis is different.
Description | The axis parameters contain different error reactions for the gantry master and slave axis. It is possible to choose between drive internal and CNC-controlled error response (see P-AXIS-00254). For gantry operation, the same setting must be used for the master and slave axes.

See also [FCT-C11// Section: Overview]

Response | Class | 1 | Warning
Solution | Class | 1 | Use the same error response (see P-AXIS-00254) for both axes.
Parameter | %1: | Logical axis number [-]
Logical axis number of the slave axis P-AXIS-00016
%2: | Error value [-]
Error response of the slave axis see P-AXIS-00254
%3: | Corrected value [-]
Expected value for error response see P-AXIS-00254
Error type | -