# Example of limitation by velocity

## Programing Example

Limitation by velocity

Dynamic characteristics used:

a_max: 1000 mm/s2

v_max: 500000µm/s

%L sub_mv

N1000 G01 G90 Y100 F500

N2000 Y-100

M29

%osc_7

N10 X[OSC ON 1ST_POS=-520 2ND_POS=520 FREQ=0.2]

N20 LL sub_mv

N30 X[OSC OFF]

N180 M30

Limited oscillating frequency due to axis acceleration

A full oscillation requires 5.164 s. The required 5 s (approx. 2500 cycles) are therefore not possible with the dynamic characteristics listed above due to the oscillating frequency of 0.2 Hz.

## Attention

When the dynamic limits are reached, an error message is output.