# Delete single distance to go applied multiple times, G01 motion

## Programing Example

Delete single distance to go applied multiple times with G01

Simulated HLI signal "delete distance to go" before end of the first “delete distance to go” is reached

%deldisttogo5

N010 X0 Y0 Z0

N020 X100 F1000

N025 G1 Z30

N029 G02 Y200 J100

N032 G01 Y220

N033 X111

N034 Y50

N035 X80

N040 X0 Y0

M30

Delete distance to go with linear motion G01