# Gearbox ratio numerator (P-AXIS-00511)

P-AXIS-00511 | Gearbox ratio numerator
Description | By default, the path resolution of an axis is set with axis parameters P-AXIS-00233 and P-AXIS-00234 , where an eventually present gearbox must be considered (load-side scaling). If the parameters P-AXIS-00511/ P-AXIS-00512 and P-AXIS-00092, P-AXIS-00362/ P-AXIS-00363 are used, the resolution of the axis can be specified related to the motor side.

The resulting resolution (R) related to the load side is calculated automatically according to the equation below:

Parameter | getriebe[i].gear_fact_num
Data type | UNS32
Data range | 1 ... MAX (UNS32)
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 1
Drive types | ----
Remarks | For possible applications, see Settings of position scaling