# Parameters

Cycle parameters | Description
@P4 | Measurement path in the X axis (incremental) Positive value, the touch probe moves in positive X direction Negative value, the touch probe moves in negative X direction
@P5 | Measurement path in the Y axis (incremental) Positive value, the touch probe moves in positive Y direction Negative value, the touch probe moves in negative Y direction
@P7 (optional) | Zero offset to be described (TCS) G54 to G59 Input without address “G” If not specified, then measurement only but no write function
@P9 (optional) | Shift the measuring point along the X axis
@P10 (optional) | Shift the measuring point along the Y axis
@P17 (optional) | Pre-position along the X axis Default value = @P4
@P18 (optional) | Pre-position along the Y axis Default value = @P5