# ID 120174

No motion programmed in pitch axis.
Description | With the thread cutting (G33) turning function, a motion path must exist in the thread pitch axis programmed with I, J or K. For more information on turning functions, see [PROG// Section: Turning functions].
Response | Class | 2 | Program abort.
Solution | Class | 6 | A real thread pitch greater than 0 must be programmed in the thread pitch axis.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of thread pitch axis.
Error type | 1, Error message from NC program.