# A rotation of the Cartesian basic coordination system (P-CHAN-00371)

P-CHAN-00371 | A rotation of the Cartesian basic coordinate system for belt synchronisation/throughfeed machining
Description | This parameter defines the rotation about the X axis for the basic coordinate system to align the machine to a conveyor belt.
Parameter | conveyor_sync.cart_t0_rot_a
Data type | REAL64
Data range | 0.0 ≤ cart_t0_rot_a ≤ 3600000.0
Dimension |
Default value | 0.0
Remarks | Parameter available in TwinCAT as of CNC Build V3.1.3108.2