# ID 20008

Feed rate in motion block is 0.
Description | At least the first motion command with interpolation (e.g. G01, G02, G03) requires a feed value (F-word). Example: Wrong: N10 G00 X0 Y0 Z0 N20 G01 X10

Correct:

N10 G00 X0 Y0 Z0

N20 G01 X10 F1000

Response | Class | 2 | Abort NC program processing. .
Solution | Class | 3 | Program the speed value using the F word.
Error type | 1, Error message from NC program.