# Parameters

Cycle parameters | Description
@P3 | Joint width
@P7 (optional) | Zero offset to be described (TCS) G54 to G59 Input without address “G” If not specified, then measurement only but no write function
@P10 (optional) | Shift the measuring point along the Y axis
@P13 (optional) | Safety clearance for pre-positioning [mm, inch] Default value = 10
@P19 | Pre-position along the Z axis
@P33 | Crossover range [mm, inch] Default value = 5