# Activation (P-AXIS-00368)

P-AXIS-00368 | Activation of axis specific command value transformation
Description | This parameter controls the general activation/deactivation of the transformation. Selection/deselection is possible only on start-up.
Parameter | trafo.command_pos.enable
Data type | BOOLEAN
Data range | 0: Transformation is disabled (default) 1: Transformation is enabled
Axis types | R
Dimension |  | R: ----
Default value | 0
Drive types | ----
Remarks |