# ID 60198

Spindle speed too small for auto. link factor calculation.
Description | When activating spindle-path coupling with automatic calculation of the coupling factor (NC-command S[FEED_LINK ON..]), the current spindle speed is less than 1*10-12 um/s. See also [[PROG// Section: Spindle feed link (FEED_LINK)] This can be caused by the spindle speed programmed in the NC program or by an override /feedhold via the HLI.
Response | Class | 6 | Program execution stop.
Solution | Class | 6 | Check override or change program; at the time of activation of the spindle-path coupling, the spindle speed must be higher.
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle
%2: | Current value [1µm/s or 0.001°/s]
Current spindle speed.
%3: | Limit value [1µm/s or 0.001°/s]
Permissible minimum value.
Error type | 1, Error message from NC program.