# ID 70332

Function DIST_CTRL ON at program end.
Description | The end of the NC program (M02/M30) was reached while distance control is still active (see [FCT-M3]). Distance control must be turned off before program end.
Response | Class | 7 | Immediate stop of the axis. The distance control is turned off.
Solution | Class | 6 | Deactivate the distance control at the program end.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Block number [-]
Block number in the NC program
Error type | 11, Error message from position controller.