# ID 110521

Homing on zero pulse is not enabled.
Description | Parameter P-AXIS-00386 was set, but the homing with zero pulse search (see P-AXIS-00084) is not active.
Response | Class | 1 | Error message output, P-AXIS-00386 is disabled.
Solution | Class | 1 | Set P-AXIS-00084 to zero.
Parameter | %1: | Logical axis number [-]
Log. Axis number (see also P-AXIS-00016).
%2: | Error value [-]
Value of P-AXIS-00084.
%3: | Current value[-]
Value of P-AXIS-00386.
%4: | Error value [-]
Corrected value of P-AXIS-00386.
Error type | 2, Error message by data transfer from parameter list into control device.