# ID 20426

Channel parameters: Axis is configured both as spindle and as path axis.
Description | During start-up, the check of the channel parameter detects that a path axis and a spindle axis have the same logical axis number P-CHAN-00035 (P-CHAN-00035, P-CHAN-00036).
Response | Class | 1 | Start-up of the control is continued.
Solution | Class | 1 | Check and change the logical axis numbers of the path axes P-CHAN-00035 and spindle axes P-CHAN-00036 in the channel parameter list. In the system, a logical axis number only may be assigned to one single axis.
Parameter | %1: | Logical axis number [-]
%2: | Current value[-]
Index of spindle has same logical axis number as path axis
Error type | 2, Error message by data transfer from parameter list into control device.