# Order of the actual position value filter of the master axis (P-AXIS-00622)

P-AXIS-00622 | Order of the actual position value filter of the master axis (throughfeed machining)
Description | The order (number of filtered values) of the actual position value filter of the master axis is defined with this parameter.
Parameter | conv_sync.order_pos_filter
Data type | UNS32
Data range | 0 ≤ order_pos_filter ≤ 1000
Axis types | T, R, S
Dimension | T: ---- | R, S: ----
Default value | 10
Drive types | ----
Remarks | Parameter available in TwinCAT as of CNC Build V3.1.3108.2