# Ignore feedhold at position correction after drive enable (P-AXIS-00356)

P-AXIS-00356 | Ignore feedhold at position correction after drive enable
Description | This parameter determines if a position correction after drive enable (see also P-AXIS-00327) can be interrupted with axis- or channel-specific feedhold. If this parameter has the value 1, a position correction can not be stopped with feedhold.
Parameter | kenngr.pos_corr_ignore_feedhold
Data type | BOOLEAN
Data range | 0/1
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
Drive types | SERCOS, Lightbus
Remarks |