# Overview

## Task

Automatic breakage check of a tool.

## Possible applications

This cycle can be used to check tools for breakage or wear during production to prevent damage to follow-on tools, for example.

## Programming

The cycles are called with the L CYCLE[..] function and the required parameters are taken directly from the NC program. A more detailed description of the call is provided in the subsections for each of the cycles.

## Parameters

The section Parameters describes the total overview of all parameters. Each cycle also has a modified parameter list which includes only the relevant parameters for the cycle.