# ID 70024

Error in SERCOS drive. Check S-0-0011 and S-0-0095.
Description | An error has occurred in the SERCOS drive. Check the ident numbers S-0-0011 and S-0-0095 to obtain information about the error that occurred, and the drive status. Consult the drive manufacturer documentation for further error diagnosis.
Response | Class | 7 | Controlled or abrupt stop of the axis
Solution | Class | 6 | Consult drive manufacturer documentation
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Drive type [-]
Drive type of concerned axis, see P-AXIS-00020
%3: | Current value [-]
SERCOS drive status
%4: | Block number [-]
Block number of the NC program where the error occurred.
%5: | Error code of drive [-]
Error type | 11, Error message from position controller.