# Name process data 'probe 2 actuated' (P-AXIS-00685)

P-AXIS-00685 | Name process data 'probe 2 actuated'
Description | This parameter defines the cyclical process data in which the drive signals in a bit that probe 2 is actuated. When one of the real-time status bits of the SERCOS status is used, this parameter must be set to 'S-0-0135' or 'S_0_135'; in all other cases it must be set to the name of the process data in the process data configuration.

If this parameter is used, enter the number of the bit used for transmission in P-AXIS-00686 .

Parameter | antr.sercos.probe_2_realtime_bits.probe_actuated.element_name
Data type | STRING
Data range | -
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | *
Drive types | SERCOS
Remarks | If the configured element name is not found in the process data configuration, the error message P-ERR-110610 and the axis parameters P-AXIS-00118 (measuring axis) and P-AXIS-00098 (kasto_axis) are reset to prevent the execution of a measurement travel or edge banding with incompletely configured probes.

* Note: The default value of variables is a blank string.