# ID 50498

The available motion path is less than the defined residual distance.
Description | With the Edge banding function,the residual path P-CHAN-00030 in the channel parameter list is reduced after the measurement signal is activated by the measuring probe. The block motion path available at this time must be greater than P-CHAN-00030.

For more information on edge banding, see [PROG// Section: Edge banding (G108)].

Response | Class | 4 | Movement stop.
Solution | Class | 0 | Either reduce P-CHAN-00030 or increase the programmed block motion path so that a residual path of at least P-CHAN-00030 is available after the response of the measurement signal.
Parameter | %1: | Current value [0.1 µm or 0.0001°]
Residual path available in the programmed measuring block.
%2: | Expected value [0.1 µm or 0.0001°]
Residual path depending on P-CHAN-00030
%3: | Current value [0.1 µm or 0.0001°]
Path distance of measurement actual positions and target positions.
%4: | Current value [0.1 µm or 0.0001°]
Motion path in current motion block.
Error type | 1, Error message from NC program.