# ID 50593

Oscillation feed is zero.
Description | The programmed oscillation axes function feedrate is too small. For more information on oscillation axes see [FCT-A8// Section: Oscillating motion dynamics].
Response | Class | 5 | Movement stop.
Solution | Class | 6 | Check feed programming, value should be > 0
Parameter | %1: | Logical axis number [-]
Logical axis number of concerned axis P-AXIS-00016.
%2: | Current value [1µm/s or 0.001°/s]
Programmed feed.
Error type | 1, Error message from NC program.