# ID 20641

Release of face turning axis not allowed during active constant cutting speed.
Description | An axis programmed in an axis exchange command is currently used with the active constant cutting speed enabled (G96) as a face turning axis P-AXIS-00015 and cannot be released. Example: Wrong: N10 G96 S63 N20 #PUT AX[X]

:

N100 G97

:

N1000 M30

Correct:

N10 G96 S63

:

N100 G97

N110 #PUT AX[X]

:

N1000 M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the program flow sequence. Before the axis exchange command, deselect active constant cutting speed (G96).
Parameter | %1: | Logical axis number [-]
Error type | 1, Error message from NC program.