# ID 21203

Channel parameters: Synchronization mode MET_SVS needs pre output time greater than or equal to NC-cycle time of control.
Description | During start-up for M-/H-functions with the synchronisation mode MET_SVS, the check of the assigned pre output time P-CHAN-00070 / P-CHAN-00107 detects that these time is smaller than the cycle time.
Response | Class | 1 | Start-up of the control is continued.
Solution | Class | 1 | In the channel parameters, check and modify the pre-output time P-CHAN-00070 / P-CHAN-00107 before the next controller start-up for the corresponding M/H function. During start-up in case of conflict the pre output time is set to cycle time and the start-up is continued.
Parameter | %1: | Current value
Number of the M-/H-function Note: For M-functions multiple ID 1 is valid. For H-functions multiple ID 2 is valid.
%2: | Error value[-]
Incorrect pre output time.
%3: | Corrected value [-]
Automatically corrected pre output time (= cycle time)
Error type | 2, Error message by data transfer from parameter list into control device.