# Position of linkpoint after axis exchange (P-TOOL-00108)

P-TOOL-00108 | Position of linkpoint after axis exchange
Description | This parameter defines the method for handling a linkpoint attached to an axis during collision consideration if this axis is no longer available in the NC channel due to axis exchange.
Parameter | wz[i].linkpoint_data.fixed
Data type | BOOLEAN
Data range | 0: Collision monitoring for this linkpoint can no longer be reliably executed. 1: Linkpoint position remains constant after axis exchange. Collision monitoring can be executed.
Dimension | ----
Default value | 0
Remarks |