# Suppression of workspace monitoring in manual operation (P-CHAN-00442)

P-CHAN-00442 | Suppression of workspace monitoring function in manual operation
Description | This parameter influences the workspace monitoring function in manual mode. As from version V3.3070.11 onwards, activating the workspace monitoring function using the NC program also simultaneously activates the workspace monitoring function in manual mode.

0: Workspace monitoring is activated as described above

1: Workspace monitoring is not activated

2: Workspace monitoring is activated; error handling is suppressed when manual mode is selected for axes located outside/within the workspace/protection area.

Parameter | suppress_workspace_monitoring_manual_mode
Data type | UNS16
Data range | 0, 1, 2
Dimension | ----
Default value | 0
Remarks | The parameter is available as of Build V3.3070.11.