# Number of probing input in drive (P-AXIS-00430)

P-AXIS-00430 | Number of probing input in drive
Description | Number of the drive digital input which is used as probing input. The input used must also be defined as probing input in the drive. See also (FCT-C4]. From CNC version V2.10.1505.26 onwards, this parameter can be used with Profidrive, CANopen and Sercos drives. If the parameter is set to 0, the following default settings are valid due to downward compatibility:

CANopen/Profidrive: Probing input 1

Sercos: Last configured probing value in the cyclic telegram

Parameter | antr.probing_input_nbr
Data type | UNS08
Data range | 0, 1, 2
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
Drive types | SERCOS, Profidrive, CANopen
Remarks |