# Measure slot in Y axis with obstacle

After positioning above the obstacle, the touch probe measures both in the positive and negative Y direction after repeated pre-positioning in the slot. The touch probe must be positioned as centrally as possible above the obstacle either manually or in automatic mode. The obstacle is located in the middle of the slot.

Measure slot in Y axis with obstacle

## Additional information

- Process (internal cycle)
- Parameters
- Syntax
- Programming example
- Output variables