# ID 120524

Intermediate point of contour mode not within start/ end/ corner point.
Description | The calculated intermediate point of the contouring curve should be within the convex envelope of the start/target and end points. This is currently not the case.
Response | Class | 2 | Warning output
Solution | Class | 1 | Check contouring curve
Parameter | %1: | Incorrect value [0.1 µm or 0.0001°]
X coordinate of intermediate point
%2: |
Y coordinate of intermediate point
%3: | Incorrect value [0.1 µm or 0.0001°]
Z coordinate of intermediate point
%4: |
Number of previous block
%5: | NC block number [0.1 µm or 0.0001°]
Number of following block
Error type | 1, Error message from NC program.