# ID 1030

Index value out of permissible range.
Description | In the start-up list, the specified axis index or channel index is greater than permissible. The maximum permissible number of channels and axes can be found in the system parameter documentation[SYSP]. Example (from start up list): sda_mds[123] ..\..\listen\sda_mds.lis

...

achs_mds[230] ..\..\listen\achsmd.lis

Correct:

sda_mds[11] ..\..\listen\sda_mds.lis

...

achs_mds[63] ..\..\listen\achsmds.lis

Response | Class | 3 | The affected parameter list is not evaluated
Solution | Class | 7 | Correct the start up list
Parameter | %1: | Current value [-]
Incorrect axis or channel index
%2: | Limit value [-]
Error type | -