# ID 70294

Correction movement was aborted.
Description | A correction movement of an axis was aborted due to one of the following reasons: During the compensation motion the PLC reset the

- MCControlBoolUnit_FollowUp signal for CNC build < 2800 (see [ HLI//Section: Axis control commands])
- lr_mc_control.follow_up for CNC Version >2800 (see [HLI// Kapitel: Axis control commands])

or

During the compensation motion the PLC reset the

- MCControlBoolUnit_ReleaseFeedhold for CNC build < 2800
- lr_mc_control.release_feedhold for CNC build > 2800

signal. [HLI// Section: Axis control commands].

The fieldbus did not deliver valid values.

Response | Class | 1 |
Solution | Class | 1 | Change PLC program or fieldbus configuration.
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Block number [-]
NC block number.
Error type | 11, Error message from position controller.