# ID 20181

Double-programmed spindle.
Description | In NC block the same spindle was programmed several times in DIN syntax. Example: Wrong: N10 G00 X0 Y0 Z0 N20 S1000 M03 X100 G01 F2000 S1500

:

`N1000 M30`

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. Remove the inadmissible spindle programming.
Error type | 1, Error message from NC program.