# ID 270059

When there is a transition, the current operation mode is not adopted.
Description | When an operation mode change is commanded, the starting operation mode does not match the current operation mode. The operation mode changeover is not carried out. See starting operation mode: [HLI// Section: Output operating mode ] for CNC build < 2800
[HLI// Section: Output operating mode ] for CNC build < 2800

The values entered in the mode state unit [HLI// Section: Operation modes] must be corrected.

Possibilities:

Enter the correct operation mode

Set the value "0" for the current operation mode. The operation mode switch will be executed regardless of the current operation mode.

Response | Class | 3 | The transition will not be done
Solution | Class | 1 | Correct the state of the starting operation mode. Create new request
Parameter | %1: |
Current operation mode
%2: |
Expected Mode
Error type | -