# ID 13165

Unknown milling direction defined.
Description | For pocket milling, it is necessary to specify a milling direction to calculate countersinking motions. This can be selected by specifying an identification number: 2: Clockwise milling (CW), 3: Counter-clockwise milling (CCW). This message is generated when an identification number other than 2 or 3 was programmed in the corresponding input parameters.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check and define the milling direction and correct input parameters.
Error type | 1, Error message from the NC program