# Drive probing input for PROBE0/1 Keyword (P-AXIS-00583)

P-AXIS-00583 | Number of the drive-specific probing input assigned to the keyword PROBE0 or PROBE1 in the command #MEAS[INPUT=..].
Description | This parameter defines which drive probing input is assigned to the keywords INPUT=PROBE0 and INPUT=PROBE1 in the command #MEAS. Assign parameters to the keywords as follows:
Keyword | Parameter
'PROBE0' | kenngr.measure.probe[0].input
'PROBE1' | kenngr.measure.probe[1].input
Example: When kenngr.measure.probe[0].input has the value 1, probing input 1 of the drive is used by the NC command #MEAS [AX=X INPUT=PROBE0] on receipt of the next probing command on the X axis. The permissible value range depends on the drive type. If the parameterised value is invalid, the error message ERR-110622 is output and the value is corrected.

If no value is parameterised for this parameter, the following default values are used:

Parameter | Default value
kenngr.measure.probe[0].input | P-AXIS-00517
kenngr.measure.probe[1].input | P-AXIS-00539 (If P-AXIS-00059 has the value 0, the value of P-AXIS-00517 is used).
Parameter | kenngr.measure.probe[i].input
Data type | SGN16
Data range | ----
Axis types | T, R
Dimension | T: ---- | R,S: ----
Default value | 0
drive types. | Simulation, Conventional, SERCOS, Terminal, Lightbus, Profidrive, CANopen
Remarks | This parameter is available as of V2.11.2808.00 and higher.