# ID 21240

G-command has no effect, because precontrol is disabled in one axis.
Description | In an axis, the feedforward cannot be switched on because it is disabled by P-AXIS-00256.
Response | Class | 1 | Continue NC program processing.
Solution | Class | 1 | P-AXIS-00256 must be set to 0 in the concerned axis .
Parameter | %1: | Current value [-]
Number of the G command
%2: | Logical axis number [-]
%3: | Error value [-]
Value of P-AXIS-00256
Error type | 1, Error message from NC program.