# ID 70333

Function DIST_CTRL ON and release axis.
Description | The axis was released (#PUT AX) but distance control is still active (see [FCT-M3]). Before axis release the distance control must be switched off.
Response | Class | 7 | Immediate stop of the axis. The distance control is turned off.
Solution | Class | 6 | Deactivate the distance control before axis release
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Block number [-]
Block number in the CNC program in which the error occurred
%3: | Error value [-]
Current correction offset of the distance control
%4: | Current value [-]
Current state of the distance control
Error type | 11, Error message from position controller.