# ID 294048

Allowed maximum force exceeded.
Description | The force probe signal is greater than"FORCE_MAX + UPPER_LIMIT_TOL" after force control "($Force[axis] > FORCE_LIM)" is switched on.
Response | Class | 7 | Dynamic braking. All active commands inhibited. Output “$ALARM_STOP” has signal level 0.
Solution | Class | 6 | Check force sensor value "$Force_act[axis]" using the menu function "Display-Variable-Single" and correct if necessary. Check force sensor and cable. Trace test group 11-Force control to determine if the controller overshoots too much.
Error type | 11, Error message from position controller.