# Parameters

Cycle parameters | Description
@P2 | Pin diameter
@P7 (optional) | Zero offset to be described (TCS) G54 to G59 Input without address “G” If not specified, then measurement only but no write function
@P9 (optional) | Shift the measuring point along the X axis
@P10 (optional) | Shift the measuring point along the Y axis
@P13 (optional) | Safety clearance for pre-positioning [mm, inch] Default value = 10
@P14 | Angle 1 to measuring point 1 relation to X+ axis [degrees] Default value = 0
@P15 | Angle 2 to measuring point 2 relation to X+ axis [degrees] Default value = 120
@P16 | Angle 3 to measuring point 3 relation to X+ axis [degrees] Default value = 240
@P19 | Pre-position along the Z axis
@P33 | Crossover range [mm, inch] Default value = 5

If @P13 is not specified, the safety clearance is set to 10mm.

Angles 1-3 must be different.